Investigation of the conformational changes of a conducting polymer in gas sensor active layers by means of polarization-modulation infrared reflection absorption spectroscopy (PM-IRRAS). Polarization-Modulation Infrared Reflection Absorption Spectroscopy (PM-IRRAS) was employed to observe the changes in the molecular conformation of poly(2-phenyl-1,4-xylylene) (PPPX) films that occurred after exposure to organic solvent vapors. The PPPX films were supported on solid matrixes by casting, spin-coating, and Langmuir-Blodgett (LB) techniques. The results show that the polymer is sensitive to the solvent vapors, which affect some of the vibration dipole moments, as detected by PM-IRRAS. The sensitivity depends on the method employed to immobilize the polymer, with more significant changes in films formed using techniques that result in a less systematically organized conformation. This feature enables the use of surface vibration spectroscopy to detect organic solvent vapors and may be applied in an artificial nose.